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Lab 5.2.2.9 – Configuring Switch Security Features
EE3009 Lab 2-2
5.2.2.9 – Configuring Switch Security Features Topology – PT (Sem B 2020/2021)


Addressing Table
	Device
	Interface
	IP Address
	Subnet Mask
	Default Gateway

	R1
	G0/0/1
	192.168.2.1
	255.255.255.0
	N/A

	S1
	VLAN 99
	192.168.2.11
	255.255.255.0
	192.168.2.1

	PC-A
	NIC
	192.168.2.3
	255.255.255.0
	192.168.2.1


Objectives
Part 1: Set up the Topology and Initialize Devices
Part 2: Configure Basic Device Settings and Verify Connectivity
Part 3: Configure and Verify SSH Access on S1
Configure SSH access.
Modify SSH parameters.
Verify the SSH configuration.
Part 4: Configure and Verify Security Features on S1
Configure and verify general security features.
Configure and verify port security.
Background / Scenario
It is quite common to lock down access and install strong security features on PCs and servers. It is important that your network infrastructure devices, such as switches and routers, are also configured with security features.
In this lab, you will follow some best practices for configuring security features on LAN switches. You will only allow SSH and secure HTTPS sessions. You will also configure and verify port security to lock out any device with a MAC address not recognized by the switch.

Set Up the Topology and Initialize Devices
Cable the network as shown in the topology.



Configure Basic Device Settings and Verify Connectivity
In Part 2, you will configure basic settings on the router, switch, and PC. Refer to the Topology and Addressing Table at the beginning of this lab for device names and address information.
Configure an IP address on PC-A.
Refer to the Addressing Table for the IP Address information.
Configure basic settings on R1.
Enter the enable mode of R1 by typing 
Router> enable
Router#
Type config t to enter global configuration mode.
Router# config t
Router(config)# 
Copy the following basic configuration and paste it to running-configuration on R1.
hostname R1
service password-encryption
line con 0
password conpass
login
logging synchronous
line vty 0 4
password vtypass
login
interface g0/0/1
 ip address 192.168.2.1 255.255.255.0
 no shutdown
end
Save the running configuration to startup configuration.
Configure basic settings on S1.
Enter the enable mode of S1 by typing 
Switch> enable
Switch#
Type config t to enter global configuration mode.
Copy the following basic configuration and paste it to running-configuration on S1.
hostname S1
service password-encryption
enable secret class
line con 0
password conpass
login
logging synchronous
line vty 0 15
password vtypass
login
exit
Create VLAN 99 on the switch and name it Management.
S1(config)# vlan 99
S1(config-vlan)# name Management
S1(config-vlan)# exit
S1(config)#
Configure the VLAN 99 management interface IP address, as shown in the Addressing Table, and enable the interface.
S1(config)# interface vlan 99
S1(config-if)# ip address 192.168.2.11 255.255.255.0
S1(config-if)# no shutdown
S1(config-if)# end
S1#
Issue the show vlan command on S1. What is the status of VLAN 99? ______________________ 
Issue the show ip interface brief command on S1. What is the status for management interface VLAN 99?
_________________________________________________________________________________
Assign ports F0/5 and F0/6 to VLAN 99 on the switch.
S1# config t
S1(config)# interface f0/5
S1(config-if)# switchport mode access
S1(config-if)# switchport access vlan 99
S1(config-if)# interface f0/6
S1(config-if)# switchport mode access
S1(config-if)# switchport access vlan 99
S1(config-if)# end
Save the running configuration to startup configuration.
Verify connectivity between devices.
From PC-A, ping the default gateway address on R1. Were your pings successful? ______________ 
From PC-A, ping the management address of S1. Were your pings successful? ______________ 
From S1, ping the default gateway address on R1. Were your pings successful? ______________ 

Configure and Verify SSH Access on S1
Configure SSH access on S1.
Enable SSH on S1. From global configuration mode, create a domain name of CCNA-Lab.com.
S1(config)# ip domain-name CCNA-Lab.com
Create a local user database entry for use when connecting to the switch via SSH. The user should have administrative level access.
Note: The password used here is NOT a strong password. It is merely being used for lab purposes.
S1(config)# username admin privilege 15 secret adminpass
Configure the transport input for the vty lines to allow SSH connections only, and use the local database for authentication.
S1(config)# line vty 0 15
S1(config-line)# transport input ssh
S1(config-line)# login local
S1(config-line)# exit
Generate an RSA crypto key using a modulus of 1024 bits.
S1(config)# crypto key generate rsa general-keys modulus 1024
The name for the keys will be: S1.CCNA-Lab.com

% The key modulus size is 1024 bits
% Generating 1024 bit RSA keys, keys will be non-exportable...
[OK] (elapsed time was 3 seconds)

S1(config)#
S1(config)# end
Verify the SSH configuration.
S1# show ip ssh
What version of SSH is the switch using? _______________________ 
How many authentication attempts does SSH allow? _______________________ 
What is the default timeout setting for SSH? _______________________ 
Modify the SSH configuration on S1.
Modify the default SSH configuration.
S1# config t
S1(config)# ip ssh time-out 75
S1(config)# ip ssh authentication-retries 2
How many authentication attempts does SSH allow? _______________________ 
What is the timeout setting for SSH? _______________________ Verify the SSH configuration on S1.
On PC-A , open an SSH connection to S1. The ip address is 192.168.2.11 and the username is  admin and adminpass is the password.
Was the connection successful? _________________________ 
What prompt was displayed on S1? Why?
_________________________________________________________________________________
_________________________________________________________________________________
_________________________________________________________________________________

Type exit to end the SSH session on S1.
Configure and Verify Security Features on S1
In Part 4, you will shut down unused ports, turn off certain services running on the switch, and configure port security based on MAC addresses. Switches can be subject to MAC address table overflow attacks, MAC spoofing attacks, and unauthorized connections to switch ports. You will configure port security to limit the number of MAC addresses that can be learned on a switch port and disable the port if that number is exceeded.
Configure general security features on S1.
Issue a show ip interface brief command on S1. What physical ports are up?
_________________________________________________________________________________
Shut down all unused physical ports on the switch. Use the interface range command.
S1(config)# interface range f0/1 – 4
S1(config-if-range)# shutdown
S1(config-if-range)# interface range f0/7 – 24
S1(config-if-range)# shutdown
S1(config-if-range)# interface range g0/1 – 2
S1(config-if-range)# shutdown
S1(config-if-range)# end
S1#
Issue the show ip interface brief command on S1. What is the status of ports F0/1 to F0/4?
_________________________________________________________________________________
Configure and verify port security on S1.
Record the R1 G0/0/1 MAC address. From the R1 CLI, use the show interface g0/0/1 command and record the MAC address of the interface.
R1# show interface g0/0/1
GigabitEthernet0/0/1 is up, line protocol is up
  Hardware is CN Gigabit Ethernet, address is 00E0.B097.0802 (bia 00E0.B097.0802)
What is the MAC address of the R1 G0/0/1 interface?
_________________________________________________________________________________
From the S1 CLI, issue a show mac address-table command from privileged EXEC mode. Find the dynamic entries for ports F0/5 and F0/6. Record them below.
F0/5 MAC address: ______________________________________________________ 
F0/6 MAC address: ______________________________________________________ 
Configure basic port security.
Note: This procedure would normally be performed on all access ports on the switch. F0/5 is shown here as an example.
From the S1 CLI, enter interface configuration mode for the port that connects to R1.
S1(config)# interface f0/5
Shut down the port.
S1(config-if)# shutdown
Note: Entering the switchport port-security command sets the maximum MAC addresses to 1 and the violation action to shutdown. The switchport port-security maximum and switchport port-security violation commands can be used to change the default behavior.
S1(config-if)# switchport port-security 
      S1(config-if)# switchport port-security maximum 1
      S1(config-if)# switchport port-security violation shutdown
Configure a static entry for the MAC address of R1 G0/0/1 interface recorded in Step 2a.
S1(config-if)# switchport port-security mac-address xxxx.xxxx.xxxx
(xxxx.xxxx.xxxx is the actual MAC address of the router G0/0/1 interface)
Note: Optionally, you can use the switchport port-security mac-address sticky command to add all the secure MAC addresses that are dynamically learned on a port (up to the maximum set) to the switch running configuration.
Enable the switch port.
S1(config-if)# no shutdown
S1(config-if)# end
Verify port security on S1 F0/5 by issuing a show port-security interface command.
S1# show port-security interface f0/5
Port Security              : Enabled
Port Status                : Secure-up
Violation Mode             : Shutdown
Aging Time                 : 0 mins
Aging Type                 : Absolute
SecureStatic Address Aging : Disabled
Maximum MAC Addresses      : 1
Total MAC Addresses        : 1
Configured MAC Addresses   : 1
Sticky MAC Addresses       : 0
Last Source Address:Vlan   : 0000.0000.0000:0
Security Violation Count   : 0
What is the port status of F0/5?
_________________________________________________________________________________
From R1 command prompt, ping PC-A to verify connectivity.
R1# ping 192.168.2.3
You will now violate security by changing the MAC address on the router interface. Enter interface configuration mode for G0/0/1 and shut it down.
R1# config t
R1(config)# interface g0/0/1
R1(config-if)# shutdown
Configure a new MAC address for the interface, using aaaa.bbbb.cccc as the address.
R1(config-if)# mac-address aaaa.bbbb.cccc
Enable the G0/0/1 interface on R1.
R1(config-if)# no shutdown
From R1 privileged EXEC mode, ping PC-A. Was the ping successful? Why or why not?
_________________________________________________________________________________
On the switch, verify port security with the following commands.
S1# show port-security
Secure Port MaxSecureAddr CurrentAddr SecurityViolation Security Action
               (Count)       (Count)        (Count)
--------------------------------------------------------------------
      Fa0/5            1           1                 1         Shutdown
----------------------------------------------------------------------
Total Addresses in System (excluding one mac per port)     :0
Max Addresses limit in System (excluding one mac per port) :8192

S1# show port-security interface f0/5
Port Security              : Enabled
Port Status                : Secure-shutdown
Violation Mode             : Shutdown
Aging Time                 : 0 mins
Aging Type                 : Absolute
SecureStatic Address Aging : Disabled
Maximum MAC Addresses      : 1
Total MAC Addresses        : 1
Configured MAC Addresses   : 1
Sticky MAC Addresses       : 0
Last Source Address:Vlan   : aaaa.bbbb.cccc:99
Security Violation Count   : 1

S1# show interface f0/5
FastEthernet0/5 is down, line protocol is down (err-disabled)
  Hardware is Fast Ethernet, address is 0cd9.96e2.3d05 (bia 0cd9.96e2.3d05)
  MTU 1500 bytes, BW 10000 Kbit/sec, DLY 1000 usec, 
     reliability 255/255, txload 1/255, rxload 1/255
<output omitted>

S1# show port-security address
                Secure Mac Address Table
------------------------------------------------------------------------
Vlan     Mac Address       Type                 Ports      Remaining Age
                                                           (mins)
----     -----------       ----                 -----   -------------
  99     30f7.0da3.1821    SecureConfigured     Fa0/5        -
-----------------------------------------------------------------------
Total Addresses in System (excluding one mac per port)     :0
Max Addresses limit in System (excluding one mac per port) :8192
On the router, shut down the G0/0/1 interface, remove the hard-coded MAC address from the router, and re-enable the G0/0/1 interface.
R1(config-if)# shutdown
R1(config-if)# no mac-address aaaa.bbbb.cccc
R1(config-if)# no shutdown
R1(config-if)# end
From R1, ping PC-A again at 192.168.2.3. Was the ping successful? _________________ 
[bookmark: _GoBack]On the switch, issue the show interface f0/5 command to determine the cause of ping failure. Record your findings.
_________________________________________________________________________________
Clear the S1 F0/5 error disabled status.
S1# config t
S1(config)# interface f0/5
S1(config-if)# shutdown
S1(config-if)# no shutdown
Note: There may be a delay while the port states converge.
Issue the show interface f0/5 command on S1 to verify F0/5 is no longer in error disabled mode.
S1# show interface f0/5
FastEthernet0/5 is up, line protocol is up (connected)
  Hardware is Fast Ethernet, address is 0023.5d59.9185 (bia 0023.5d59.9185)
  MTU 1500 bytes, BW 100000 Kbit/sec, DLY 100 usec,
     reliability 255/255, txload 1/255, rxload 1/255
From the R1 command prompt, ping PC-A again. The ping should be successful.
If not, troubleshoot.

 Save your Packet Tracer file and upload to Canvas.  
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