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Tutorial 10
1. Using JK FFs and with the minimum number of states to design a counter with counting sequence: 0,4,2,1,6 and repeat.  State whether the circuit is a self started circuit.


2. Design a sequential circuit with two JK FFs, A & B, and two inputs, x & E. if E=0, the circuit remains in the same state regardless of the value of x.  When E = 1 and x = 1, the circuit goes through the state transitions from 00 to 01 to 10 to 11 back to 00, and repeats.  When E =1 and x = 0, the circuit goes through the state transitions from 00 to 11 to 10 to 01 back to 00, and repeats.


3. Using a synchronous binary counters as shown in Figure 1, design and draw a counter to generate the following repeating sequences 2 to 9 repeatedly for a free running clock.

                                   [image: ]
Figure 1.



4. Write the VHDL code for a D-FF with (i) asynchronous Preset and Clear, and (ii) synchronous Preset and Clear. 
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