EE3315: Polling questions and answers for lecture on 18 Feb 2020
1.  The use of hierarchy in routing tables can ________ the size of the routing tables.	
	a.  reduce *
	b.  increase
	c.  both a and b
	d.  none of the above
			
2.  ____________ is a group of networks and routers under the authority of a single administration.	
	a.  An autonomous system *
	b.  An area
	c.  a and b
	d.  none of the above
			
3.  In Routing Information Protocol (RIP), each node periodically shares its routing table with _________ and whenever there is a change.	
	a.  every other node
	b.  its immediate neighbors *
	c.  one neighbor
	d.  none of the above
			
4.  In ________, we assume that there is one node (or more) in each autonomous system that acts on behalf of the entire autonomous system.	
	a.  distant vector routing (e.g. RIP)
[bookmark: _GoBack]	b.  path vector routing (e.g. BGP) *
	c.  link state routing (e.g. OSPF)
	d.  none of the above

